1. **Beta Version 71.06.44.02 T5**

|  |  |  |  |
| --- | --- | --- | --- |
| **Models** | **Software Version** | **Firmware Name** | **Building time** |
| MGE1300 | 71.06.44.02 T5 | package\_71064402\_T5\_3000c | 2024-12-25 19:02:03 |

1. **Version relevance**
	1. Base version 71.06.44.02 T4 2024-10-09
2. **Bug Fixing**
	1. Transferred the cause of reason from SIP-T to SS7.
	2. Fix the bug when using SIP-T for SS7->IP call and re-routing to IP, the 2nd INVITE without ISUP-Body.
3. **Improvements**

4.1 Support the feature of Call route PSTN->PSTN.

1. **Others**

The following image is device upgraded.



1. **Note**

Null.